This is part of Family API which allow to create dual-os version of program runs under OS/2 and DOS

Note: This is legacy API call. It is recommended to use 32-bit equivalent

VioEndPopUp

This call is issued by the application when it no longer requires the temporary screen obtained through a previous VioPopUp call.

Syntax

VioEndPopUp (VioHandle)

Parameters

VioHandle (HVIO) - input : A reserved word of 0s.

Return Code

rc (USHORT) - return:Return code descriptions are:

0 NO_ERROR

405 ERROR_VIO_NO_POPUP

436 ERROR_VIO_INVALID_HANDLE

Remarks

When the application issues a VioEndPopUp call, all video calls are directed to the application's normal video buffer.

PM Considerations

An error is returned if issued with a non-zero handle.

Bindings

C

#define INCL_VIO USHORT rc = VioEndPopUp(VioHandle); HVIO VioHandle; /* Vio device handle */ USHORT rc; /* return code */

MASM

EXTRN VioEndPopUp:FAR INCL_VIO EQU 1 PUSH WORD VioHandle ;Vio device handle CALL VioEndPopUp Returns WORD

Related Functions

VioPopUp

http://www.edm2.com/index.php/VioEndPopUp_(OS/2_1.x)