INT 21 - DOS 2+ - GET COUNTRY-SPECIFIC INFORMATION

AH = 38h

–DOS 2.x–

AL = 00h get current-country info
DS:DX -> buffer for returned info (see #01398,#01399)

Return: CF set on error

AX = error code (02h)
CF clear if successful
AX = country code (MS-DOS 2.11 only)
buffer at DS:DX filled